io7m | single-page | multi-page
3.25. vm-run
Previous
3. Command-Line Interface
Up
3.27. vm-update-boot-configurations
Next
3.26

# vm-set

- 3.26. vm-set
  - 3.26.1. Name
  - 3.26.2. Description
  - 3.26.3. Example

3.26.1

## Name

1
vm-set - Set virtual machine configuration flags
3.26.2

## Description

1
The vm-set command sets configuration flags for virtual machines.
2

### 3.26.2.2 Parameters

Parameter | Type | Required | Description
--- | --- | --- | ---
--configuration | Path | false | The path to the configuration file (environment variable: $WAXMILL_CONFIGURATION_FILE)
--machine | UUID | true | The ID of the virtual machine
--verbose | Log Level | false | Set the minimum logging verbosity level.
--include-guest-memory-cores | Boolean | false | Include guest memory in core files.
--yield-on-HLT | Boolean | false | Yield the virtual CPU thread when a HLT instruction is detected.
--exit-on-PAUSE | Boolean | false | Force the guest virtual CPU to exit when a PAUSE instruction is detected.
--generate-acpi-tables | Boolean | false | Generate ACPI tables. Required for FreeBSD/amd64 guests.
--disable-mptable-generation | Boolean | false | Disable MP table generation.
--force-msi-interrupts | Boolean | false | Force virtio PCI device emulations to use MSI interrupts instead of MSI-X interrupts.
--guest-apic-is-x2apic | Boolean | false | The guest's local APIC is configured in x2APIC mode.
--rtc-is-utc | Boolean | false | RTC keeps UTC time.
--ignore-unimplemented-msr | Boolean | false | Ignore accesses to unimplemented Model Specific Registers.
--wire-guest-memory | Boolean | false | Enable/disable wiring of guest memory.

3.26.3

## Example

1

### 3.26.3.1 Example

    $ waxmill vm-set \
      --machine 538a90e4-d50d-4511-8643-ae418279bac4 \
      --wire-guest-memory true

3.25. vm-run
Previous
3. Command-Line Interface
Up
3.27. vm-update-boot-configurations
Next
io7m | single-page | multi-page